LumiSoft Net Help
LastSR Property
Namespaces ► LumiSoft.Net.RTP ► RTCP_Packet_ReportBlock ► LastSR
Gets or sets The middle 32 bits out of 64 in the NTP timestamp (as explained in Section 4) received as part of the most recent RTCP sender report (SR) packet from source SSRC_n. If no SR has been received yet, the field is set to zero.
Declaration Syntax

C# | Visual Basic | Visual C++ | F#

    public uint LastSR { get; set; }

    Public Property LastSR As UInteger
    	Get
    	Set

    public:
    property unsigned int LastSR {
    	unsigned int get ();
    	void set (unsigned int value);
    }

    member LastSR : uint32 with get, set

Property Value
UInt32

Assembly: LumiSoft.Net (Module: LumiSoft.Net.dll) Version: 4.5.5510.19119