LumiSoft Net Help
SIP_t_Directive..::..DirectiveType Enumeration
Namespaces ► LumiSoft.Net.SIP.Message ► SIP_t_Directive ► SIP_t_Directive..::..DirectiveType
Proccess directives. Defined in rfc 3841 9.1.
Declaration Syntax

C# | Visual Basic | Visual C++ | F#

    public enum DirectiveType

    Public Enumeration DirectiveType

    public enum class DirectiveType

    type DirectiveType

Members

Member | Description
--- | ---
Proxy | This directive indicates whether the caller would like each server to proxy request.
Redirect | This directive indicates whether the caller would like each server to redirect request.
Cancel | This directive indicates whether the caller would like each proxy server to send a CANCEL request to forked branches.
NoCancel | This directive indicates whether the caller would NOT want each proxy server to send a CANCEL request to forked branches.
Fork | This type of directive indicates whether a proxy should fork a request.
NoFork | This type of directive indicates whether a proxy should proxy to only a single address. The server SHOULD proxy the request to the "best" address (generally the one with the highest q-value).
Recurse | This directive indicates whether a proxy server receiving a 3xx response should send requests to the addresses listed in the response.
NoRecurse | This directive indicates whether a proxy server receiving a 3xx response should forward the list of addresses upstream towards the caller.
Parallel | This directive indicates whether the caller would like the proxy server to proxy the request to all known addresses at once.
Sequential | This directive indicates whether the caller would like the proxy server to go through all known addresses sequentially, contacting the next address only after it has received a non-2xx or non-6xx final response for the previous one.
Queue | This directive indicates whether if the called party is temporarily unreachable, caller wants to have its call queued.
NoQueue | This directive indicates whether if the called party is temporarily unreachable, caller don't want its call to be queued.

Assembly: LumiSoft.Net (Module: LumiSoft.Net.dll) Version: 4.5.5510.19119