LumiSoft Net Help
RTP_Address Constructor (ip, dataPort, controlPort, ttl)
Namespaces ► LumiSoft.Net.RTP ► RTP_Address ► RTP_Address(IPAddress, Int32, Int32, Int32)
Multicast constructor.
Declaration Syntax

C# | Visual Basic | Visual C++ | F#

    public RTP_Address(
    	IPAddress ip,
    	int dataPort,
    	int controlPort,
    	int ttl
    )

    Public Sub New (
    	ip As IPAddress,
    	dataPort As Integer,
    	controlPort As Integer,
    	ttl As Integer
    )

    public:
    RTP_Address(
    	IPAddress^ ip,
    	int dataPort,
    	int controlPort,
    	int ttl
    )

    new :
            ip : IPAddress *
            dataPort : int *
            controlPort : int *
            ttl : int -> RTP_Address

Parameters

ip (IPAddress)
  Multicast IP address.

dataPort (Int32)
  RTP data port.

controlPort (Int32)
  RTP control port. Usualy this is dataPort + 1.

ttl (Int32)
  RTP control port. Usualy this is dataPort + 1.

Exceptions

Exception | Condition
--- | ---
ArgumentNullException | Is raised when ip is null reference.
ArgumentException | Is raised when any of the arguments has invalid values.

Assembly: LumiSoft.Net (Module: LumiSoft.Net.dll) Version: 4.5.5510.19119