LumiSoft Net Help
DelaySinceLastSR Property
Namespaces ► LumiSoft.Net.RTP ► RTCP_Packet_ReportBlock ► DelaySinceLastSR
Gets or sets the delay, expressed in units of 1/65536 seconds, between receiving the last SR packet from source SSRC_n and sending this reception report block. If no SR packet has been received yet from SSRC_n, the DLSR field is set to zero.
Declaration Syntax

C# | Visual Basic | Visual C++ | F#

    public uint DelaySinceLastSR { get; set; }

    Public Property DelaySinceLastSR As UInteger
    	Get
    	Set

    public:
    property unsigned int DelaySinceLastSR {
    	unsigned int get ();
    	void set (unsigned int value);
    }

    member DelaySinceLastSR : uint32 with get, set

Property Value
UInt32

Assembly: LumiSoft.Net (Module: LumiSoft.Net.dll) Version: 4.5.5510.19119