LumiSoft Net Help
SIP_StatusCodeType Enumeration
Namespaces ► LumiSoft.Net.SIP.Stack ► SIP_StatusCodeType
Specifies SIP status code type. Defined in rfc 3261.
Declaration Syntax

C# | Visual Basic | Visual C++ | F#

    public enum SIP_StatusCodeType

    Public Enumeration SIP_StatusCodeType

    public enum class SIP_StatusCodeType

    type SIP_StatusCodeType

Members

Member | Description
--- | ---
Provisional | Request received, continuing to process the request. 1xx status code.
Success | Action was successfully received, understood, and accepted. 2xx status code.
Redirection | Request must be redirected(forwarded). 3xx status code.
RequestFailure | Request contains bad syntax or cannot be fulfilled at this server. 4xx status code.
ServerFailure | Server failed to fulfill a valid request. 5xx status code.
GlobalFailure | Request cannot be fulfilled at any server. 6xx status code.

Assembly: LumiSoft.Net (Module: LumiSoft.Net.dll) Version: 4.5.5510.19119